Vader WWTP must comply with the following requirements as a condition of Agreed Order #\_\_\_\_\_\_:

1. All biosolids must be screened through a 3/8” bar screen or other approved method before they are transported off site for beneficial use.
2. Seeding of decommissioned basin 3 must take place at a time and in a fashion to allow enough growth to prevent significant erosion from taking place during fall rains. If this is not possible to achieve, other methods of preventing residual biosolids from eroding out of the lagoon area must be used and approved by Ecology.
3. Timing of sampling from basins actively receiving flow is important. If the time period between sample collection and start time of biosolids removal in a basin exceeds the times listed below additional samples may be needed prior to removal:
   * VAR: 60 days
   * Fecal Coliform: 45 days
   * Pollutants: 60 days
4. Sufficient removal of biosolids from Basin 3 must be reviewed and approved by ecology before any additional materials are added such as topsoil, soil amendments or seed.
5. Non-significant changes or amendments to the above plans can be required or approved by Ecology as necessary. Any significant changes (as defined in WAC 173-308-080 Definitions) may require notification of interested parties, posting the site for public notice, and a 30 day comments period per WAC 173-308-310 (13).